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Chapter 26 – OFF-STREET PARKING AND LOADING REGULATIONS
Section 26.05. Parking lot site requirements.
Whenever the required off-street parking requires the building of a parking lot, and whenever a parking lot is built, such parking lot shall be laid out, constructed, and maintained in accordance with the following requirements: 
[1]	Lighting facilities shall be so arranged that light is reflected away from adjacent properties. 
[2]	The parking lot shall be adequately drained. 
[3]	Along lot lines of a parking area which abut a residential district, a dense planting of trees and shrubsParking Lots shall be established on a strip of land not less than eight (8) feet in width adjacent to the districts, and such planting shall not be less than six (6) feet in height and a substantial bumper rail of wood, metal, or concrete shall be installed on the inside of the planting strip except where topography or other conditions would make the bumper rail unnecessary. 
[4]	Abounded by a raised curb of at least six (6) inches shall be erected along all property lines, except for driveway openings and those lot lines abutting residential districts where the requirements in Section 26.05[3] shall prevail. 
[54]	No sign, whether permanent or temporary, shall be placed within the public right-of-way. Signs and planting strips shall be arranged so that they do not obstruct visibility for drivers or pedestrians. 
[6]	Landscaping	
 [5]	In parking lots for shopping centers and large-scale retail, as well as in any commercial parking lotlots of twenty (20) or more spaces or more, the following standards shall apply: 
(a)	Parking Islands. Parking islands shall be provided withthroughout a parking lot and located no more than one hundred (100) feet from another parking island and at the terminus of all rows of parking. Each parking island shall: 
(i) Be at least five (5) feet wide and a minimum of two hundred (200) square feet in area for single parking rows, and four hundred (400) square feet for double parking rows; and 
(ii) Contain at least one (1) shade/canopy tree or two (2) intermediate trees per 200 square feet of area.
     (b) 	All landscaped areas in or adjacent to a parking lot shall be protected from
vehicular damage by either a raised curb at least six (6) inches in height, or a wall at least thirty (30) inches in height. 
(c) All interior landscaping coveringlandscaped areas of the parking lot not less than five (5) percent of the total area of the parking lot. The primarydedicated to trees or to
 preservation of existing vegetation, including parking islands, shall be landscaped with grass, ground cover, shrubs, or other appropriate landscape material should be trees and the treatment. 
(d) Sand or other pavement shall not be used as landscape areas should be treatment. 

[6]	Alternative Interior Landscape Option. If a parking lot that was in existence prior to [effective date of these amendments] needs to be expanded but cannot reasonably dispersed throughout comply with the siterequirements of this subsection, an alternative design may be submitted to the Commission for approval. 
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